**Annex 3: Technical Specifications**

Fill in the way: in the column "yes" or "no" if it is a column yes, enter „yes”, and the column no leave blank, and if it is a "no" column, enter "no" in that column and leave column "yes" empty.

Offers in which technical specifications are not precise can be discarded.

The offer must be clear enough to make a simple comparison between the requested and the offered specifications.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Stone cutting machine | | Yes | | No | |
| Possibility of cutting granite and marble |  | |  | | |
| Cutting height 1900 mm |  | |  | | |
| Cutting length 3400 mm |  | |  | | |
| Cutting width 1800 mm |  | |  | | |
| Automatic cutting control |  | |  | | |
| Setting the working parameters (speed, number of cuts and cutting speeds) |  | |  | | |
| Turning table for blocks |  | |  | | |
| Granite cutting wire |  | |  | | |
| Marble cutting wire |  | |  | | |
| Water pressure sensor |  | |  | | |
| Heating system in control cabinet |  | |  | | |
| Regulation the height of water sprayer |  | |  | | |
| Racks stands that provide stone blocks |  | |  | | |
| Anchoring machine |  | |  | | |
| Wheelchair with rotating table |  | |  | | |
| Connector rail |  | |  | | |
| Wheel Drive (For Trolleys - Automatic) |  | |  | | |
| Outdoor case system |  | |  | | |
| Control cabinet placed separately from the poust |  | |  | | |
| Safety fences around the work bench |  | |  | | |
| Power supply 400 V |  | |  | | |
| Assembly of the machine and commissioning by the manufacturer |  | |  | | |
| Stroj za poliranje kamena | | Yes | | | No |
| Work surface length 200000mm |  | |  | | |
| Work surface width 3200 mm |  | |  | | |
| Possibility of polishing granite and marble with plugs included |  | |  | | |
| Possibility of polishing boards of different thicknesses in the same operation |  | |  | | |
| Possibility of polishing plates of irregular shapes |  | |  | | |
| Automatic start with a light start or the same value |  | |  | | |
| Assembly of the machine and commissioning by the manufacturer |  | |  | | |
| Power supply 400 V |  | |  | | |
| Compressed air 0.5 MPa |  | |  | | |
| Engine head 11 KW |  | |  | | |
| Spindle speed 420 rpm |  | |  | | |
| Pneumatic head (0.05-0.1) MPa |  | |  | | |
| Training for two employees | | Yes | | No | |
| Duration 1 day |  | |  | | |
| Duration 8 hours |  | |  | | |
| Minimum 2 employees |  | |  | | |
| Venue - Customer Space |  | |  | | |

In **\_\_\_\_\_\_\_\_\_\_\_\_, \_\_\_\_\_\_\_\_\_\_\_\_** year.

Offeror:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

For offeror:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

(readily enter the first and last name of the authorized person of the economic operator)

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

(Place stamp here)  (Authorized signature of the authorized person of the economic operator)