**GUMIIMPEX - GUMI RECIKLAŽA I PROIZVODNJA d.o.o.**

**Pavleka Miškine 64/c**

**Varaždin, Croatia/Hr**

Varaždin, 29.09. 2021.

**1ST . MODIFICIATION OF INVITATION TO TENDER/**

**1. IZMJENA POZIVA NA DOSTAVU PONUDA**

**Contracting Authority has published 15.09.2021. on the website** [**www.strukturnifondovi.hr**](http://www.strukturnifondovi.hr) **Invitation to Tender with all accompanying annexes for procurement DUST EXTRACTION AND FILTRATION SYSTEM WITH MOUNTING.**

***Naručitelj je dana 15.09. 2021. na stranici*** [***www.strukturnifondovi.hr***](http://www.strukturnifondovi.hr) ***objavio Poziv na dostavu ponuda sa pripadajućim prilozima za nabavu SUSTAV ZA OTPRAŠIVANJE I FILTRIRANJE S MONTAŽOM.***

**Contracting Authority hereby modifies Invitation to Tender in the following sections:/**

***Naručitelj ovime mijenja Poziv na dostavu ponuda u sljedećim dijelovima:***

1. **17. SUBMISSION OF BIDS/*DOSTAVA PONUDE***

**17. SUBMISSION OF BIDS/*DOSTAVA PONUDE***

**The offer shall be delivered at latest by 12:00h (CET), 12.10.2021. in envelope to the following address:/ *Ponude moraju biti dostavljene u zatvorenoj omotnici neposredno naručitelju ili poštanskom pošiljkom najkasnije do 12:00h (CET), 12.10.2021. na sljedeću adresu*:**

**GUMIIMPEX - GUMI RECIKLAŽA I PROIZVODNJA d.o.o.**

**Pavleka Miškine 64/c, Varaždin, Croatia/*Hrvatska***

**Procurement identification number: 2/2021 / *Evidencijski broj nabave: 2/2021***

**Subject of procurement: Dust extraction and filtration system with mounting / *Naziv nabave: Sustav za otprašivanje i filtriranje s montažom***

**Tender and documentation enclosed with tender will not be returned to the tenderers.**

**Tenderer may, by the expiry of the deadline for the submission of tenders, submit a modification and / or amendment to the tender. A modification and / or amendment to the tender is submitted in the same way as the basic tender along with an indication that the modification and / or amendment of the offer is to be made. In this case, the tender is opened in reverse order of receipt and the delivery time is considered to be the delivery of the last version of the tender modification.**

**Tenderer may, by the written notice, withdraw from the tender submitted by the end of the tender deadline. The written statement is submitted in the same way as a tender with a mandatory indication that it is a waiver of the offer. In this case, unopened tender is returned to the tenderer. /**

***Ponuda i dokumentacija u prilogu ponude ne vraćaju se ponuditeljima.***

***Ponuditelj može do isteka roka za dostavu ponuda dostaviti izmjenu i/ili dopunu ponude. Izmjena i/ili dopuna ponude dostavlja se na isti način kao i osnovna ponuda s obveznom naznakom da se radi o izmjeni i/ili dopuni ponude. U tom se slučaju ponude otvaraju obrnutim redoslijedom zaprimanja, a vremenom zaprimanja smatra se dostava posljednje verzije izmjene ponude.***

***Ponuditelj može do isteka roka za dostavu ponude pisanom izjavom odustati od svoje dostavljene ponude. Pisana izjava se dostavlja na isti način kao i ponuda s obveznom naznakom da se radi o odustajanju od ponude. U tom slučaju neotvorena ponuda se vraća ponuditelju.***

**Tenders that arrive after the deadline for submitting tenders will not be subject to an evaluation of tenders. / *Ponude koje pristignu nakon isteka roka za dostavu ponuda neće biti predmetom ocjene ponuda.***

**Opening tenders is not public. /**

***Otvaranje ponuda nije javno.***

1. **Annex 2. Techinical Specifications is amended in following points:/  
   *Prilog 2. Tehničke specifikacije mijenjaju se u sljedećim točkama:***

**Point 1. line 28 regarding BAG FILTER, ex protection, which read/ *Točka 1. redak 28 vezano za VREČASTI FILTER, ex zaštitu, koja je glasila***

|  |  |
| --- | --- |
| Technical specification /  Tehničke karakteristike | **Minimum 6 explosion venting panels in accordance with Atex directives.**  Minimalno 6 ploče za zaštitu kod eksplozije u skladu s Atex direktivama. |

**Changes to/*Mijenja se u*:**

|  |  |
| --- | --- |
| Technical specification /  Tehničke karakteristike | **Minimum 6 explosion venting panels in accordance with ATEX 22 CAT 3D or equal EX PROTECTION.**  Minimalno 6 ploče za zaštitu kod eksplozije u skladu s ATEX 22 CAT 3D ili jednakovrijednoj EX ZAŠTITI. |

**Point 2. line 31 regarding FAN, ex protection, which read/ *Točka 2. redak 31 vezano za VENTILATOR, ex zaštitu, koja je glasila***

|  |  |
| --- | --- |
| Technical specification /  Tehničke karakteristike | **Centrifugal fan, ATEX 22 medium pressure or equal, made in steel S235JR or equal, painted. Coupled in transmission with the electric motor complete of: basement with rubber vibration dampers, statically and dynamically balanced impeller and three phase asynchronous motor, inspection door on the case and coupling for the condensate discharge.**  /  Centrifugalni ventilator, ATEX 22 srednji tlak ili jednakovrijedno, izrađen od čelika S235JR ili jednakovrijedno, obojan. Spojen u prijenos s elektromotorom kompletno od temelja s gumenim prigušivačima vibracija, statički i dinamički uravnoteženim rotorom i trofaznim asinkronim motorom, kontrolnim vratima na kućištu i spojkom za ispuštanje kondenzata. |

**Changes to/*Mijenja se u*:**

|  |  |
| --- | --- |
| Technical specification /  Tehničke karakteristike | **Centrifugal fan, with ATEX 22 CAT 3D or equal EX PROTECTION, made in steel S235JR or equal, painted. Coupled in transmission with the electric motor complete of: basement with rubber vibration dampers, statically and dynamically balanced impeller and three phase asynchronous motor, inspection door on the case and coupling for the condensate discharge.**  / Centrifugalni ventilator, sa ATEX 22 CAT 3D ili jednakovrijednom EX ZAŠTITOM, izrađen od čelika S235JR ili jednakovrijedno, obojan. Spojen u prijenos s elektromotorom kompletno od temelja s gumenim prigušivačima vibracija, statički i dinamički uravnoteženim rotorom i trofaznim asinkronim motorom, kontrolnim vratima na kućištu i spojkom za ispuštanje kondenzata. |

**These changes are published in separat document as modifications:**

**- 1. Modification-Poziv-na-dostavu-ponuda-Sustav-za-otprašivanje-i-filtriranje-s-**

**montažom**

**- 1. Modification\_Annex 2\_Tehnical Specification\_Sustav-za-otprašivanje-i-filtriranje-s-**

**montažom**

**which represent a consolidated version with modifications included, marked in red.**

**The rest of the Invitation to Tender remains unchanged./**

***Predmetne izmjene objavljuju se u zasebnim dokumentima kao izmjena:***

***- 1. Modification-Poziv-na-dostavu-ponuda-Sustav-za-otprašivanje-i-filtriranje-s-montažom***

***- 1. Modification\_Annex 2\_Tehnical Specification\_Sustav-za-otprašivanje-i-filtriranje-s-montažom***

***koji predstavljaju pročišćenu verziju sa uključenim izmjenama koje su označene crvenom bojom.***

***Ostatak Poziva ostaje neizmijenjen.***

**Contracting Authority/*Naručitelj*:**

**GUMIIMPEX - GUMI RECIKLAŽA I PROIZVODNJA d.o.o.**