**Prilog V. / Annex V.**

**TEHNIČKE SPECIFIKACIJE / TECHNICAL SPECIFICATIONS**

**Grupa 2 / Lot 2**

**Dvoglava pila za rezanje EUX mehanizama /**

**Double-head saw for cutting eux mechanisms**

NAPOMENA: Ponuditelj nudi predmet nabave putem ove tablice Tehničkih specifikacija koja će činiti dio ponude.

Ponuditelj je dužan ponuditi svaku stavku kako je tražena u stupcu 2. Tražene karakteristike.

Ponuđeni predmet nabave je pravilan i prihvatljiv samo ako ispunjava sve zahtijevane uvjete i svojstva. Nije prihvatljivo precrtavanje ili korigiranje stavke navedene u stupcu 2. Tražene karakteristike. Ponuditelj obavezno popunjava stupac 3. «Ponuđene karakteristike» definirajući detaljno tehničke specifikacije ponuđene robe (napomena: ponuditelj popunjava tehničke specifikacije upisujući točne karakteristike ponuđene robe, izbjegavajući pri tome popunjavanje stupca samo riječima kao što su npr. „zadovoljava“ , „DA“, „jednakovrijedno traženom“ ili „odgovara traženom“). Ponude ponuditelja koji ne popune tehničke specifikacije sa točnim karakteristikama ponuđene robe mogu biti odbačene.

Zahtjevi definirani Tehničkim specifikacijama predstavljaju minimalne tehničke karakteristike koje ponuđena roba mora zadovoljavati, ukoliko nije drugačije navedeno, te se iste ne smiju mijenjati od strane ponuditelja.

NOTE: These Technical specifications must be filled in by the Tenderer and will be submitted as a part of the offer.

The tenderer is obliged to offer each item as required in column 2. Required technical specification.

Offered item is acceptable only if it meets all the required conditions and properties. No amendments or corrections to the items listed in column 2 Required technical specification are allowed. Tenderer is required to fill column 3 " Offered technical specification " defining in detail the technical specifications of the goods offered (note: the tenderer fills the technical specifications with exact characteristics of the goods offered, while avoiding filling column with only words such as, "satisfactory", "Yes", "equivalent" or" as required"). Offer from tenderers who do not fill the technical specifications with the correct characteristics of the goods offered can be rejected.

|  |  |  |
| --- | --- | --- |
| **1. Red. br. / No.** | **2. Tražene karakteristike / Required technical specifications** | **3. Ponuđene karakteristike / Offered technical specifications** |
| **1.** | **Dvoglava pila za rezanje EUX mehanizama /**  **Double-head saw for cutting eux mechanisms** |  |
|  | **Proizvođač / Producer:** |  |
|  | **Model / Type:** |  |
|  | **Količina / Quantity: 1** |  |
|  | snaga motora za pilu 3-5 kw / saw motor power 3-5 kw |  |
|  | broj okretaja motora lista pile 2800 1/min (minimalno) / saw motor speed 2800 rpm (minimum) |  |
|  | promjer lista pile 550-600 mm / saw blade diameter 550-600 mm |  |
|  | duljina minimalnog reza 200-300 mm / length of minimum cut 200-300 mm |  |
|  | brzina pomaka lista pile 30-60 mm/s / saw blade speed 30-60 mm/s |  |
|  | brzina pomaka nosača profila 20-40 m/min minimalno / shift speed of the profile carrier 20-40 m/min minimum |  |
|  | iskoristiv pritisak 6-8 bar / usable pressure 6-8 bar |  |
|  | Jamstvo za ispravnost prodane stvari 2 godine minimalno. Jamstveni period započinje od dana prihvata robe i usluga. / Guarantee for correctness of sold goods 2 years minimum. The warranty period starts from the day of acceptance of the delivered goods and services. |  |

\_\_\_\_\_\_\_\_\_\_\_\_\_\_, \_\_/\_\_/2021.

ZA PONUDITELJA/ ON BEHALF OF THE TENDERER

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

(ime, prezime i potpis ovlaštene osobe/ name, signature of the authorised representative)