**Prilog V. / Annex V.**

**TEHNIČKE SPECIFIKACIJE / TECHNICAL SPECIFICATIONS**

**Grupa 4 / Lot 4**

**Pedane za transport gotovih proizvoda /**

**Transport rack for finished products**

NAPOMENA: Ponuditelj nudi predmet nabave putem ove tablice Tehničkih specifikacija koja će činiti dio ponude.

Ponuditelj je dužan ponuditi svaku stavku kako je tražena u stupcu 2. Tražene karakteristike.

Ponuđeni predmet nabave je pravilan i prihvatljiv samo ako ispunjava sve zahtijevane uvjete i svojstva. Nije prihvatljivo precrtavanje ili korigiranje stavke navedene u stupcu 2. Tražene karakteristike. Ponuditelj obavezno popunjava stupac 3. «Ponuđene karakteristike» definirajući detaljno tehničke specifikacije ponuđene robe (napomena: ponuditelj popunjava tehničke specifikacije upisujući točne karakteristike ponuđene robe, izbjegavajući pri tome popunjavanje stupca samo riječima kao što su npr. „zadovoljava“ , „DA“, „jednakovrijedno traženom“ ili „odgovara traženom“). Ponude ponuditelja koji ne popune tehničke specifikacije sa točnim karakteristikama ponuđene robe mogu biti odbačene.

Zahtjevi definirani Tehničkim specifikacijama predstavljaju minimalne tehničke karakteristike koje ponuđena roba mora zadovoljavati, ukoliko nije drugačije navedeno, te se iste ne smiju mijenjati od strane ponuditelja.

NOTE: These Technical specifications must be filled in by the Tenderer and will be submitted as a part of the offer.

The tenderer is obliged to offer each item as required in column 2. Required technical specification

Offered item is acceptable only if it meets all the required conditions and properties. No amendments or corrections to the items listed in column 2 Required technical specification are allowed. Tenderer is required to fill column 3 "Offered technical specification" defining in detail the technical specifications of the goods offered (note: the tenderer fills the technical specifications with exact characteristics of the goods offered, while avoiding filling column with only words such as, "satisfactory", "Yes", "equivalent" or "as required"). Offer from tenderers who do not fill the technical specifications with the correct characteristics of the goods offered can be rejected.

|  |  |  |
| --- | --- | --- |
| **1. Red. br. / No.** | **2. Tražene karakteristike / Required technical specifications** | **3. Ponuđene karakteristike / Offered technical specifications** |
| **1.** | **Pedane za transport gotovih proizvoda /**  **Transport rack for finished products** |  |
|  | **Proizvođač / Producer:** |  |
|  | **Model / Type:** |  |
|  | **Količina / Quantity: 50** |  |
|  | dimenzije: dužina 1700-2500 mm, širina 800-1500 mm, visina 1700-2300 mm / dimensions: length 1700-2500 mm, width 800-1500 mm, height 1700-2300 mm |  |
|  | osnovni okvir 40-60/40-60/2-3 mm / basic frame 40-60/40-60/2-3 mm |  |
|  | težina 300 kg maksimalno / weight 300 kg maximum |  |
|  | noge za viličar – 4 kom / leg forklift - 4 pcs |  |
|  | vodoravni profil 2-4 kom / horizontal profile 2-4 pcs |  |
|  | vertikalni profil 6-8 kom / vertical profile 6-8 pcs |  |
|  | Jamstvo za ispravnost prodane stvari minimalno 1 godina. Jamstveni period započinje od dana prihvata robe i usluga. / Guarantee for correctness of sold goods 1 year minimum. The warranty period starts from the day of acceptance of the delivered goods and services |  |

\_\_\_\_\_\_\_\_\_\_\_\_\_\_, \_\_/\_\_/2021.

ZA PONUDITELJA/ ON BEHALF OF THE TENDERER

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

(ime, prezime i potpis ovlaštene osobe/ name, signature of the authorised representative)