**Prilog V. / Annex V.**

**TEHNIČKE SPECIFIKACIJE / TECHNICAL SPECIFICATIONS**

**Grupa 5 / Lot 5**

**Elektro viličar 2,5 T /**

**Forklift truck 2,5t elektro**

NAPOMENA: Ponuditelj nudi predmet nabave putem ove tablice Tehničkih specifikacija koja će činiti dio ponude.

Ponuditelj je dužan ponuditi svaku stavku kako je tražena u stupcu 2. Tražene karakteristike.

Ponuđeni predmet nabave je pravilan i prihvatljiv samo ako ispunjava sve zahtijevane uvjete i svojstva. Nije prihvatljivo precrtavanje ili korigiranje stavke navedene u stupcu 2. Tražene karakteristike. Ponuditelj obavezno popunjava stupac 3. «Ponuđene karakteristike» definirajući detaljno tehničke specifikacije ponuđene robe (napomena: ponuditelj popunjava tehničke specifikacije upisujući točne karakteristike ponuđene robe, izbjegavajući pri tome popunjavanje stupca samo riječima kao što su npr. „zadovoljava“ , „DA“, „jednakovrijedno traženom“ ili „odgovara traženom“). Ponude ponuditelja koji ne popune tehničke specifikacije sa točnim karakteristikama ponuđene robe mogu biti odbačene.

Zahtjevi definirani Tehničkim specifikacijama predstavljaju minimalne tehničke karakteristike koje ponuđena roba mora zadovoljavati, ukoliko nije drugačije navedeno, te se iste ne smiju mijenjati od strane ponuditelja.

NOTE: These Technical specifications must be filled in by the Tenderer and will be submitted as a part of the offer.

The tenderer is obliged to offer each item as required in column 2. Required technical specification

Offered item is acceptable only if it meets all the required conditions and properties. No amendments or corrections to the items listed in column 2 Required technical specification are allowed. Tenderer is required to fill column 3 "Offered technical specification" defining in detail the technical specifications of the goods offered (note: the tenderer fills the technical specifications with exact characteristics of the goods offered, while avoiding filling column with only words such as, "satisfactory", "Yes", "equivalent" or "as required"). Offer from tenderers who do not fill the technical specifications with the correct characteristics of the goods offered can be rejected.

|  |  |  |
| --- | --- | --- |
| **1. Red. br. / No.** | **2. Tražene karakteristike / Required technical specifications** | **3. Ponuđene karakteristike / Offered technical specifications** |
| **1.** | **Elektro viličar 2,5 T /****Forklift truck 2,5t elektro** |  |
|  | **Proizvođač / Producer:** |  |
|  | **Model / Type:** |  |
|  | **Količina / Quantity: 1** |  |
|  | bočni pomak, zvučni signal, skupljanje i širenje vilica / lateral displacement, audible signal, shrinking and expanding forks |  |
|  | nosivost 2000 kg minimalno/ load capacity 2000 kg minimum |  |
|  | Kran-triplex / kran triplex |  |
|  | nosivost na maksimalnoj visini dizanja minimalno 1800 kg / load capacity at maximum lift height minimum of 1800 kg |  |
|  | visina dizanja 5200-5500 mm / lifting height 5200-5500 mm |  |
|  | kotači-poliuteran /polyurethane wheels |  |
|  | pozicioner vilica (skupljanje širenje) 550-1600 mm minimalno / hydraulic fork movement 500-1600 mm minimum |  |
|  | baterija minimalno 48 V, 460 Ah / battery minimum 48 V, 460Ah |  |
|  | sustav za centralno nadolijevanje vode / central water recharge system |  |
|  | brzina 13-20 km/h / speed 13-20/km/h |  |
|  | senzor protiv udara / shock sensor |  |
|  | upravljanje svim funkcijama preko joysticka / control of all functions via joystick |  |
|  | Jamstvo za ispravnost prodane stvari minimalno 3 godine ili 3000 radnih sati. Jamstveni period započinje od dana prihvata robe i usluga. / Guarantee for correctness of sold goods minimum 3 years or 3000 working hours. The warranty period starts from the day of acceptance of the delivered goods and services |  |

\_\_\_\_\_\_\_\_\_\_\_\_\_\_, \_\_/\_\_/2021.

 ZA PONUDITELJA/ ON BEHALF OF THE TENDERER

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 (ime, prezime i potpis ovlaštene osobe/ name, signature of the authorised representative)