**OMIAL NOVI d.o.o.**

**Zakučac 11, Omiš**

**21310 Croatia/*Hrvatska***

Omiš, 5.5. 2021.

**1ST . MODIFICIATION OF INVITATION TO TENDER/**

**1. IZMJENA POZIVA NA DOSTAVU PONUDA**

**Contracting Authority has published 4.5.2021. on the website** [**www.strukturnifondovi.hr**](http://www.strukturnifondovi.hr) **Invitation to Tender with all accompanying annexes for procurement Equipment for 100% surface control of lacquered foil./**

***Naručitelj je dana 4.05. 2021. na stranici*** [***www.strukturnifondovi.hr***](http://www.strukturnifondovi.hr) ***objavio Poziv na dostavu ponuda sa pripadajućim prilozima za nabavu Oprema za 100% nadzor kvalitete površine lakirane folije.***

**Contracting Authority hereby modifies Invitation to Tender in the following sections:/**

***Naručitelj ovime mijenja Poziv na dostavu ponuda u sljedećim dijelovima:***

**Annex 2. Technical Specifications is amended in following point:/  
*Prilog 2. Tehničke specifikacije mijenja se u sljedećoj točki:***

* **Point 4 . which read/ *Točka 4. koja je glasila***

|  |  |
| --- | --- |
| **Operator Workstation and software functions / Upravljačka radna stanica i programske funkcije / package/komplet** | |
| Technical specification /  Tehničke karakteristike | Master PC for data storage with 2 x 500 Gbyte hard disks(redundant data storage) / Glavno računalo za pohranjivanje podataka s 2 x 1 Tbyte tvrdim diskom(redundantni zapis podataka). |
| 24" touchscreen monitor, keyboard, mouse / 24" monitor na dodir, tipkovnica, miš |
| I/O interfaces (4 output / 4 input signals / I/O sučelje (4 izlaza/4 ulaza) |
| Displaying Camera Data as Live View as 1D plot, for evaluation of recipe selection and material properties / Prikazivanje podataka kamere kako Live View tako i 1D crteža, za procjenu odabira recepata i svojstava materijala |
| Recipe Manager to select right inspection data based on the material properties / Upravitelj recepata za odabir pravih podataka o inspekciji na temelju svojstava materijala |
| Software for image processing/ program za obradu slike |
| rule based classifier / osnovna klasifikacija grešaka |
| self-learning classifier for defects/ self-learning klasifikator grešaka. |
| Training for one person in the company from which the equipment comes, in which participants gain an overview over web inspection system,the training lasts for 3 days/ Obuku za jednu osobu u firmi odakle dolazi oprema,gdje će osoba biti upoznata sa svim mogućnostima sustava u trajanju od 3 dana. |
| Interface to system for thin coat weight measurements on metallic substrates,for showing 1D trendgraph along lenght of roll/ Sučelje prema sustavu za mjerenje nanosa na metalnim podlogama a za prikazivanje 1D grafa nanosa po duljini role. |
| If barcode is missing or 2x in row same barcode appear at the software system, the system will generate an alarm at the traffic light/ ako barkod nedostaje ili se isti učita 2 puta uzastopno sustav će generirati alarm koji će se prikazivati na semaforu |

**Changes to/*Mijenja se u*:**

|  |  |
| --- | --- |
| **Operator Workstation and software functions / Upravljačka radna stanica i programske funkcije / package/komplet** | |
| Technical specification /  Tehničke karakteristike | Master PC for data storage with 2 x 500 Gbyte hard disks(redundant data storage) / Glavno računalo za pohranjivanje podataka s **2 x 500 Gigabajta** tvrdim diskom(redundantni zapis podataka). |
| 24" touchscreen monitor, keyboard, mouse / 24" monitor na dodir, tipkovnica, miš |
| I/O interfaces (4 output / 4 input signals / I/O sučelje (4 izlaza/4 ulaza) |
| Displaying Camera Data as Live View as 1D plot, for evaluation of recipe selection and material properties / Prikazivanje podataka kamere kako Live View tako i 1D crteža, za procjenu odabira recepata i svojstava materijala |
| Recipe Manager to select right inspection data based on the material properties / Upravitelj recepata za odabir pravih podataka o inspekciji na temelju svojstava materijala |
| Software for image processing/ program za obradu slike |
| rule based classifier / osnovna klasifikacija grešaka |
| self-learning classifier for defects/ self-learning klasifikator grešaka. |
| Training for one person in the company from which the equipment comes, in which participants gain an overview over web inspection system,the training lasts for 3 days/ Obuku za jednu osobu u firmi odakle dolazi oprema,gdje će osoba biti upoznata sa svim mogućnostima sustava u trajanju od 3 dana. |
| Interface to system for thin coat weight measurements on metallic substrates,for showing 1D trendgraph along lenght of roll/ Sučelje prema sustavu za mjerenje nanosa na metalnim podlogama a za prikazivanje 1D grafa nanosa po duljini role. |
| If barcode is missing or 2x in row same barcode appear at the software system, the system will generate an alarm at the traffic light/ ako barkod nedostaje ili se isti učita 2 puta uzastopno sustav će generirati alarm koji će se prikazivati na semaforu |

**These changes are published in separate documents as modifications:**

**Annex 2- TECHNICAL SPECIFICATIONS\_1st Modification**

**which represent a consolidated version with modifications included, marked in red.**

**The rest of the Invitation to Tender remains unchanged.**

**Taking into account that the deadline for submission of tenders is not shorter than 8 (eight) days from the date of publication of this modification, deadline for submission is not extended./**

***Predmetne izmjene objavljuju se u zasebnim dokumentima kao izmjena:***

***Annex 2- TECHNICAL SPECIFICATIONS\_1st Modification***

***koji predstavljaju pročišćenu verziju sa uključenim izmjenama koje su označene crvenom bojom.***

***Ostatak Poziva ostaje neizmijenjen.***

***Uzimajući u obzir da rok za dostavu ponude nije kraći od 8 (osam) dana od dana objave ove izmjene, isti se ne produljuje.***

**Contracting Authority/*Naručitelj*:**

**OMIAL NOVI d.o.o.**